Food truck details

The truck drives fine, usually takes 3 turns for her to fire up.

Run on propane(mounted under carriage), the steering column will have to be rebuilt, the keys were lost so the door also needs a new lock (we have been leaving the passenger window slightly open to gain entry)

The exhaust manifold was replaced, and the distributor cap will pop if driven over 2000rpms.

Does overheat in the summer when hot. Ideally to be stationary would be ideal or short trips. Hills are an issue she is heavy and slow

New battery located under driver seat

Purchaser will need a NSC number as this commercial truck is over 5000(GVRW) and will need to go to weigh scales when travelling – if driven n- we tried to reduce weight to avoid this, but the checker plate prevents this

The roof top windows need replacement (ravens tried to break in)

All hook up hoses/power cables – 4 prong or 3 prong dependants on power supply – shore power or generator

**The equipment**

Cooler fridge, the compressor was changed in 2022. Needs coolant added to resume operation.

The freezer was purchased in 2023.

Hot water tank replaced in 2021, 300-gallon grey water tank

2 deep fryers are in good working condition. The left one is also the pilot and needs to be always lite when operating.

100litre propane tank

The BBQ is in good working condition

The flat top is in good working condition, the ignition switches do not work (never have when purchased from community futures) you must use long matches to light. The hole without the wire is where it lights. We light the right side and middle; the left does not work (never has since purchased)

The fire compression system is top notch and was recharged in 2022.

Hood fan motor was replaced in 2023.

Mounted potato chopper.

4 sinks (requirement from Northern Health)

Northern health certified 2022.